|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Infrastructure Type | Location | Address | Structure | Warranty | Notes.1 |
| Structures | F3432 | PORTER RD | WETWELL LINER | Accepted | N/A |
| Structures | F3432 | PORTER RD | WETWELL | Accepted | N/A |
| Mechanical | F3432 | PORTER RD | WETWELL | Accepted | Guide rail brackets for both pumps 1 & 2 are not properly secured and gromets need to be tightened. Accepted 1-23/25 |
| Electrical | F3432 | PORTER RD | WETWELL | Accepted | N/A |
| Site | F3432 | PORTER RD | WETWELL | Accepted | N/A |
| Health and Safety | F3432 | PORTER RD | WETWELL | Accepted | N/A |